**ADDENDUM #1**

1. **Bid Documents Due:** Bid Documents must be delivered to the Derek Sullivan, Town Administrator at [dsullivan@wareham.ma.us](mailto:dsullivan@wareham.ma.us) and Patty Neal Assistant to the Town Administrator at [pneal@wareham.ma.us](mailto:pneal@wareham.ma.us) by 12:00 p.m. on June 1, 2023.
2. **Dewatering:** The ground water table is 2’ below the ground surface. All labor, materials and equipment for dewatering shall be included in the pricing.
3. **Chart of soil borings and depths:**

West End Drilling has installed and developed three 6” soil observation bores:

Site #1: Wankinquoah & Swifts Beach Rd

Augered 50

41.7376386-70.7195809

0’-4’ Mixed silt/Clay

4’-17’ Silt/Clay

17’-50’ Fine sand/Yellow brown

Site #2: Bayview & Wankinquoah

Augered 40

41.7373361-70.7206916

15’-25’ Fine clean sand

25’-40’ Fine sand and silt

Site #3: Wankinquoah Ave & Barnes St

Augered 22

41.7369055-70.7221635

0’-2’ Medium sand

2’-4’ Medium sand

4’-16’ Silt

16’-22’ Medium sand

1. **Insertion shafts-**furnish and supply all labor, material and equipment to stabilize the bottoms of the insertion shafts for the safe support of men and equipment. Safety is priority #1. Bidder will bid based on 1’ (one foot) of structural blend stone to create the work floor in the pit. If more is needed it will be based on Fair Market Price of material and trucking from a local yard. All material removed from work site will be moved approximately 1 mile to storage site to be returned to fill pit as needed. All unusable soils will be left at that site and removed from the property of the Town of Wareham and will become the property of the Town of Wareham. The Contractor will cover all unusable soils with tarps and it will be maintained by the Town of Wareham until moved.